The 9 character long code numbers and 4 character short codes in the file names and short product names (For example: Long code: 222-110-020, Short Code: A060, Short product Name: GM631CC) are unique to each product and all it is the same in our documents

It will be easy to find product images if one of them is written (for example, the A060 short code) in the search bar on our website and in PDF documents (searched with "CTRL + F").

These codes and some explanations are written “RED” in this document and you may need to delete all “RED” articles before giving this document to the official institutions!!!!

**MOBILE TABLE (Wide) WITH DRAWER**

**TECHNICAL SPECIFICATIONS**

1. The upper part of the table should be made of AISI 304 stainless steel, the other parts should be smooth round and disinfectant resistant stainless furnace so that their joints (welded) should be smooth and resistant to impacts.
2. There should be a telescopic rail system mounted under the working table for the Sealcut Pouchmaking devices, which throw the bags produced from the front. 1 STU Autoclave basket, which can be purchased optionally, should be mounted on this rail or deep or narrow drawers made of MDF, which can be purchased optionally, should be installed. When these baskets or MDF drawers are not used, they should be pushed under the table (with drawer logic.
3. The dimensions of the table should be 600 x 800 x 700-1050 mm [Length x Width x Height] and its weight should not exceed 20 Kg. The height of the table should be adjustable without the need for any tools.
4. The table should have four wheels, two of them with brakes.
5. The table must be guaranteed against factory defects for 2 years.
6. **The following optional devices / accessories must match the dimensions and specifications of the above product:**
   * **Autoclave basket (Large) {A072 GM500KC}:** The autoclave basket in size 1STU should be able to be attached to the telescopic drawer rail system under the front desk of the above station. This basket should be removed when requested or pushed under the table (with drawer logic) when not in use.
   * **MDF Drawer (Small) {A073 GM250KW}:** This small MDF Drawer can be mounted on the above station, which can be attached to the telescopic drawer rail system underneath the work table, to transport the sealed packages or to be used as a material drawer.
   * **MDF Drawer (Large) {A074 GM500KW}:** This large MDF Drawer can be mounted on the above station, which can be attached to the telescopic drawer rail system underneath the work table, to transport the sealed packages or to be used as a material drawer.
   * **Shelf (Wide) {A055 GM632CCS}:** In order to gain space in the work area, the above device must be placed on the lower part of this shelf which can be mounted on the "Mobile Table" or any table and any product up to 100 Kg or "Manual Roll Cutting Apparatus" below must be placed on the mobile table above.
   * **Automatic SealCut PouchMaker Device {40GM GM6LCSFV or 30GM GM5LCSFV}:** These devices that cut and close 8 pieces of 5cm or 43cm sterilization rolls in different widths in the desired length and number should be placed on the mobile table above.
   * **Sorting Table {A025 GM450TC}:** It should be AISI 304 stainless steel, this sorting table should be compatible with the mobile table above, preventing the dispensing of the pouches thrown out of the Automatic SealCut PouchMaker device.
   * **Rotary Sealer with Printer {10GM GM11L1PV or 20GM GM16L1PV}:** When closing the edges of all bags without width limitation, these devices that write the desired information to the bag with their internal printer should be placed on the table above (under the shelf, if any).
   * **Front table (Wide) {A020 GM111TC}:** It should be made of AISI 304 stainless steel, this front plate which prevents the pouch from wearing out as a support to the pouch passing through the device should be compatible with the mobile table above.
   * **Roller Conveyor (Long) {A040 GM140RTL}:** It should have a height-adjustable plastic bearing. This conveyor, which prevents the pouch from abrasion by supporting heavy pouches passing through the device, must be compatible with the mobile table above.
   * **Manual Roll Cutting & Sealer (Extra Wide) {07GM GM60MSN}:** This device, which has the function of manually cutting and sealing the sterilization rolls up to 60cm or rolls of different widths in the desired length at the same time, should be useful on the table above.
   * **Manual Roll Cutting & Sealer (Wide) {06GM GM40MSN}:** This device, which has the function of manually cutting and sealing the sterilization rolls up to 40cm or rolls of different widths in the desired length at the same time, should be useful on the table above.
   * **Magnified Lamp {A125 GM125MGL}:** This illuminated magnifying glass, which provides maintenance and control of surgical instruments, should be mounted on the above working table.
   * **Document Folder {A120 GM120DHL}:** This document holder, which allows maintenance instructions and auxiliary documents to be easily readable, should be mounted on the worktable above.