**AUTOCLAVE BASKET**

**TECHNICAL SPECIFICATIONS**

**For Workstations and Mobile Tables**

1. Must be in the form of AISI 304 stainless steel braided basket.
2. The main carrier should be 6mm and others in diameter and 3mm, and there should be no traces of welding, burrs, and no opening in the autoclave.
3. 570 X 280 X 260 mm. It should be at max. 2,5 Kg.
4. Hand-free spaces for holding / carrying on the long sides of the basket.